IGNITER DISABLE

POWER

COMPUTER

SOLENOID

SYSTEM ACTIVE

IGNITER CONTINUITY

TEST (20 mA)

ARM

IGNITER ENABLE